Door Handle Rusting

-

Citroen XM

The door handles of all XM’s are held in place by three screws. The heads of these screws are prone to rust. When you need to remove a handle I have found that at least 1 of the screw heads breaks off and another lets the screw driver rotate in the head. So the full handle assembly has to be taken out of the door to remove the broken screws. My local Citroen dealer cannot find a part number for the screws. Screw head size is important if the handle rubber trim is to fit  tightly to the door.  I have used ScrewFix  M4 x 10 Prodrive Pan machine screws, cat no 86939 using a little squirt of waxoil. These screws are about £2 for 50 and are stainless steel which should solve the rusting problem.  

I took a few photos  which are below.

Fig 1, 2 & 3 show the rusted screws in situ. Figs 4, 5 & 6 show how the handle comes apart, the bit that fit inside the door and how the rusted screws fall to bits under my heavy handed attention. 
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