Record of Equipment for the Cargo Ship Safety Certificate (Form C)

This Record shall be permanently attached to the Cargo Ship Safety Equipment Certificate

RECORD OF EQUIPMENT FOR COMPLIANCE WITH THE INTERNATIONAL CONVENTION FOR THE SAFETY OF LIFE AT SEA, 1974, AS MODIFIED BY THE PROTOCOL OF 1988 RELATING THERETO

1
Particulars of ship

Name of ship

Distinctive number or letters

Minimum number of persons with required qualifications to operate the radio installations

2
Details of life-saving appliances

	1
Total number of persons for which life-saving appliances are provided

	

	
	Port side
	Starboard side

	Total number of lifeboats

2.1
Total number of persons accommodated by them

2.2
Number of totally enclosed lifeboats (regulation III/31 and LSA Code, section 4.6)

2.3
Number of lifeboats with a self-contained air support system (regulation III/31 and LSA Code, section 4.8)

2.4
Number of fire-protected lifeboats (regulation III/31 and LSA Code, section 4.9)

2.5
Other lifeboats

2.5.1
Number

2.5.2
Type

2.6
Number of freefall lifeboats

.6.1
Totally enclosed (regulation III/31 and LSA Code, section 4.7)

2.6.2
Self-contained (regulation III/31 and LSA Code, section 4.8)

2.6.3
Fire-protected (regulation III/31 and LSA Code, section 4.9)

3
Number of motor lifeboats included in the total lifeboats shown above

3.1
Number of lifeboats fitted with searchlights

4
Number of rescue boats

4.1
Number of boats which are included in the total lifeboats shown above

5
Liferafts

5.1
Those for which approved launching appliances are required

5.1.1
Number of liferafts

5.1.2
Number of persons accommodated by them

5.2
Those for which approved launching appliances are not required

5.2.1
Number of liferafts

5.2.2
Number of persons accommodated by them

5.3
Number of liferafts required by regulation III/31.1.4

6
Number of lifebuoys

7
Number of lifejackets

8
Immersion suits

8.1
Total number

8.2
Number of suits complying with the requirements for lifejackets

9
Number of thermal protective aids

10
Radio installations used in life-saving appliances

10.1
Number of radar transponders

10.2
Number of two-way VHF radiotelephone apparatus
	
	


3
Details of radio facilities

	Item
	Actual provision

	1
Primary systems

1.1
VHF radio installation

1.1.1
DSC encoder

1.1.2
DSC watch receiver

1.1.3
Radiotelephony

1.2
MF radio installation

1.2.1
DSC encoder

1.2.2
DSC watch receiver

1.2.3
Radiotelephony


1.3
MF/HF radio installation

1.3.1
DSC encoder


1.3.2
DSC watch receiver


1.3.3
Radiotelephony


1.3.4
Direct-printing telegraphy

1.4
INMARSAT ship earth station

2
Secondary means of alerting


3
Facilities for reception of maritime safety information


3.1
NAVTEX receiver


3.2
EGC receiver


3.3
HF direct-printing radiotelegraph receiver


4
Satellite EPIRB


4.1
COSPAS-SARSAT


4.2
INMARSAT


5
VHF EPIRB


6
Ship's radar transponder
	


4
Methods used to ensure availability of radio facilities (regulations IV/15.6 and 15.7)

4.1
Duplication of equipment 

4.2
Shore-based maintenance 

4.3
At-sea maintenance capability 

5
Details of navigational systems and equipment

	Item
	Actual provision

	1.1
	Standard magnetic compass

	

	1.2
	Spare magnetic compass2
	

	1.3
	Gyro-compass2
	

	1.4
	Gyro-compass heading repeater2
	

	1.5
	Gyro-compass bearing repeater2
	

	1.6
	Heading or track control system2
	

	1.7
	Pelorus or compass bearing device

	

	1.8
	Means of correcting heading and bearings
	

	1.9
	Transmitting heading device (THD)3
	

	2.1
	Nautical charts/Electronic chart display and information system (ECDIS)

	

	2.2
	Back-up arrangements for ECDIS
	

	2.3
	Nautical publications
	

	2.4
	Back-up arrangements for electronic nautical publications
	

	3.1
	Receiver for a global navigation satellite system/terrestrial radionavigation system3, 4
	

	3.2
	9 GHz radar3
	

	3.3
	Second radar (3 GHz/ 9 GHz4)3
	

	3.4
	Automatic radar plotting aid (ARPA)3
	

	3.5
	Automatic tracking aid3
	

	3.6
	Second automatic tracking aid3
	

	3.7
	Electronic plotting aid3
	

	4
	Automatic identification system (AIS)
	

	5
	Voyage data recorder (VDR)
	

	6.1
	Speed and distance measuring device (through the water)3
	

	6.2
	Speed and distance measuring device (over the ground in the forward and athwartship direction)3
	

	7
	Echo-sounding device3
	

	8.1
	Rudder, propeller, thrust, pitch and operational mode indicator3
	

	8.2
	Rate-of-turn indicator3
	

	9
	Sound reception system3
	

	10
	Telephone to emergency steering position3
	

	11
	Daylight signalling lamp3
	

	12
	Radar reflector3
	

	13
	International Code of Signals
	


THIS IS TO CERTIFY that this Record is correct in all respects

Issued at 
(Place of issue of the Record)
(Date of issue)

(Signature of duly authorized official issuing the Record)

(Seal or stamp of the issuing authority, as appropriate)
� Excluding those required by the LSA Code, paragraphs 4.1.5.1.24, 4.4.8.31 and 5.1.2.2.13.


� Alternative means of meeting this requirement are permitted under regulation V/19. In case of other means they shall be specified.


� Alternative means of meeting this requirement are permitted under regulation V/19. In case of other means they shall be specified.


� Delete as appropriate





