Record of equipment for the Cargo Ship Safety Equipment Certificate (Form E)

This Record shall be permanently attached to the Cargo Ship Safety Equipment Certificate

RECORD OF EQUIPMENT FOR COMPLIANCE WITH THE INTERNATIONAL CONVENTION FOR THE SAFETY OF LIFE AT SEA, 1974, AS MODIFIED BY THE PROTOCOL OF 1988 RELATING THERETO

1
Particulars of ship

Name of ship

Distinctive number or letters

2
Details of life-saving appliances

	1
Total number of persons for which life-saving appliances are provided
	

	
	Port side
	Starboard side

	2
Total number of lifeboats

2.1
Total number of persons accommodated by them

2.2
Number of totally enclosed lifeboats (regulation III/31 and LSA Code, section 4.6)

2.3
Number of lifeboats with a self-contained air support system (regulation III/31 and LSA Code, section 4.8)

2.4
Number of fire-protected lifeboats (regulation III/31 and LSA Code, section 4.9)

2.5
Other lifeboats

2.5.1
Number

2.5.2
Type
	
	


	2.6
Number of freefall lifeboats

2.6.1
Totally enclosed (regulation III/31 and LSA Code, section 4.7)

2.6.2
Self-contained (regulation III/31 and LSA Code, section 4.8)

2.6.3
Fire-protected (regulation III/31 and LSA Code, section 4.9)

3
Number of motor lifeboats (included in the total lifeboats shown above)

3.1
Number of lifeboats fitted with searchlights

4
Number of rescue boats

4.1
Number of boats which are included in the total lifeboats shown above

5
Liferafts

5.1
Those for which approved launching appliances are required

5.1.1
Number of liferafts

5.1.2
Number of persons accommodated by them

5.2
Those for which approved launching appliances are not required

5.2.1
Number of liferafts

5.2.2
Number of persons accommodated by them


5.3
Number of liferafts required by regulation III/31.1.4

6
Number of lifebuoys

7
Number of lifejackets

8
Immersion suits

8.1
Total number

8.2
Number of suits complying with the requirements for lifejackets

9
Number of thermal protective aids

10
Radio installations used in life-saving appliances

10.1
Number of radar transponders

10.2
Number of two-way VHF radiotelephone apparatus
	


3
Details of navigational systems and equipment

	Item
	Actual provision

	1.1
	Standard magnetic compass

	

	1.2
	Spare magnetic compass*
	

	1.3
	Gyro-compass*
	

	1.4
	Gyro-compass heading repeater*
	

	1.5
	Gyro-compass bearing repeater*
	

	1.6
	Heading or track control system*
	

	1.7
	Pelorus or compass bearing device*
	

	1.8
	Means of correcting heading and bearings
	

	1.9
	Transmitting heading device (THD)*
	

	2.1
	Nautical charts/Electronic chart display and information system (ECDIS)

	

	2.2
	Back-up arrangements for ECDIS
	

	2.3
	Nautical publications
	

	2.4
	Back-up arrangements for electronic nautical publications
	

	3.1
	Receiver for a global navigation satellite system/ terrestrial radionavigation system*†
	

	3.2
	9 GHz radar*
	

	3.3
	Second radar (3 GHz/ 9 GHz†)*
	

	3.4
	Automatic radar plotting aid (ARPA)*
	

	3.5
	Automatic tracking aid*
	

	3.6
	Second automatic tracking aid*
	

	3.7
	Electronic plotting aid*
	

	4
	Automatic identification system (AIS)
	

	5
	Voyage data recorder (VDR)
	

	6.1
	Speed and distance measuring device (through the water)*
	

	6.2
	Speed and distance measuring device (over the ground in the forward and athwartship direction)*
	

	7
	Echo-sounding device

	

	8.1
	Rudder, propeller, thrust, pitch and operational mode indicator*
	

	8.2
	Rate-of-turn indicator*
	

	9
	Sound reception system*
	

	10
	Telephone to emergency steering position*
	

	11
	Daylight signalling lamp*
	

	12
	Radar reflector*
	

	13
	International Code of Signals
	


THIS IS TO CERTIFY that this Record is correct in all respects

Issued at 
(Place of issue of the Record)
(Date of issue)

(Signature of duly authorized official issuing the Record)

(Seal or stamp of the issuing authority, as appropriate)

� Excluding those required by the LSA Code, paragraphs 4.1.5.1.24, 4.4.8.31 and 5.1.2.2.13.


� Alternative means of meeting this requirement are permitted under regulation V/19. In case of other means they shall be specified.


� Delete as appropriate


� Alternative means of meeting this requirement are permitted under regulation V/19. In case of other means they shall be specified.





